NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Burundi  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:**  Burundi Bureau of Standards and Quality Control (BBN) Boulevard de la Tanzanie N° 500 BP: 3535 Bujumbura, Burundi Tel: +25722221815/+25722221577 E- Mail: [info@bbnburundi.org](mailto:info@bbnburundi.org) Website: [www.bbnburundi.org](http://www.bbnburundi.org)  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****X],** **5.7.1 [****],** **other****:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Paints and varnishes (ICS 87.040) |
| **5.** | **Title, number of pages and language(s) of the notified document:** Two-pack epoxy zinc phosphate weldable primer — Specification (18 page(s), in English) |
| **6.** | **Description of content:** This Draft East African Standard specifies requirements, methods of sampling and test for two-pack epoxy zinc phosphate weldable primer. This material is used as a base coat for the painting of steel structures /equipment where corrosion protection and chemical resistance under marine atmospheric conditions are required. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Consumer information, labelling; Quality requirements; Harmonization |
| **8.** | **Relevant documents:**   * ISO 9117-1, Paints and varnishes — Drying tests — Part 1: Determination of through-dry state and through-dry time * ISO 9117-3, Paints and varnishes — Drying tests — Part 3: Surface-drying test using ballotini * ISO 11890-1, Paints and varnishes — Determination of volatile organic compound (VOC) content —Part 1: Difference method * ISO 15528, Paints, varnishes and raw materials for paints and varnishes — Sampling * ISO 17132, Paints and varnishes — T-bend test * KS 1992, Two-pack epoxy zinc phosphate weldable primer — Specification |
| **9.** | **Proposed date of adoption:** To be determined  **Proposed date of entry into force:** 6 months from adoption |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:**  Documentation and Information Centre Division at BBN Boulevard de la Tanzanie N° 500 BP: 3535 Bujumbura, Burundi Tel: +25722221815 or +25722221577 E- Mail: [info@bbnburundi.org](mailto:info@bbnburundi.org) Website: [www.bbnburundi.org](http://www.bbnburundi.org)  <https://bbnburundi.org/wp-content/uploads/2021/05/DEAS_1052_-2021_Epoxy-zinc-phosphate-primer.pdf> |